**LIST OF TABLES**

|  |  |  |
| --- | --- | --- |
| **TABLE NUMBER** | **NAME OF THE TABLE** | **PAGE NO.** |
| 5.1 | Features of ATMEGA328P IC | 46 |
| 5.2 | Pin Description of Arduino Nano | 47 |
| 7.1 | List of AT command | 60 |
| 7.2 | AT – Test AT startup | 61 |
| 7.3 | AT+RST – Restart module | 61 |
| 7.4 | AT+CWMODE – Wi-Fi mode | 62 |
| 7.5 | AT+CWLAP – List available Access Points | 63 |
| 7.6 | AT+CWJAP – Connect to AP (Access Point) | 65 |
| 7.7 | AT+CWQAP – Disconnect from AP | 67 |
| 7.8 | AT+CWSAP – Configuration of softAP mode | 68 |
| 7.9 | AT+CWLIF – IP of stations | 68 |
| 7.10 | AT+CIPSTA- Set IP address of station | 69 |
| 7.11 | AT+CIPSTART – Establish TCP | 70 |
| 7.12 | AT+CIPSEND – Send data | 71 |
| 9.1 | Pin description of ADXL345 | 74 |
| 9.2 | REGISTER MAP | 75 |
| 9.3 | Register POWER\_CTL | 75 |