**LIST OF FIGURE**

|  |  |  |
| --- | --- | --- |
| **FIGURE NUMBER** | **NAME OF THE FIGURE** | **PAGE NO.** |
|  | ATMEGA328P Arduino Nano | 1 |
|  | Wi-Fi ESP 8266 | 1 |
|  | 3-Axis Analog Accelerometer | 1 |
|  | Collision zone detected | 4 |
| 2.2 | Identification of collision | 5 |
| 4.1 | Sending of data | 6 |
| 4.2 | Green coloured Virtual Boundary | 6 |
| 4.3 | Wi-Fi P2P Communication | 7 |
| 4.4 | Wi-Fi P2P Connections and nodes | 7 |
| 4.5 | Avoidance and detection of occurrence of collision | 8 |
| 5.1 | ATMEGA328 QIP (Quad in Package) IC | 43 |
| 5.2 | ATMEGA328 QIP (Quad in Package) IC pin detail | 43 |
| 5.3 | Arduino Nano pin detail | 46 |
| 5.4 | 3-Axis analog Accelerometer | 47 |
| 5.5 | 3-Axis digital Accelerometer | 47 |
| 5.6 | ADXL345 axis | 48 |
| 5.7 | ESP 8266 Wi-Fi Module | 50 |
| 5.8 | Arduino IDE (Integrated Development Environment) | 51 |
| 6.1 | Parallel to Serial Communication | 55 |
| 6.2 | Arduino Nano Interfacing with ESP8266 Module | 56 |
| 6.3 | OUTPUT of Program1 | 58 |
| 7.1 | Wi-Fi ESP8266 Module | 60 |
| 7.2 | OUTPUT of AT+CWMODE? | 62 |
| 7.3 | OUTPUT of AT+CWLAP | 63 |
| 7.4 | OUTPUT of AT+CWJAP? | 66 |
| 7.5 | OUTPUT of AT+CWQAP | 67 |